The below instructions are for the application Network manager. Small deviances may appear when using other applications.

1. Add a new WiFi network to the list of configurations.
2. Set the name of the network (SSID: karinthy) on the "Wi-Fi" tab.
3. On the Wi-Fi Security tab, you have to set the type of encryption. Choose "WPA & WPA2 Enterprise".
4. After that, choose "Tunneled TLS" authentication, and check "No CA certificate is required" so that the computer does not check the certificate of our server. Inner authentication should be set to "MSCHAPv2". Finally, type your "karinthy" username and password in the relevant fields. You can then connect to the network.